%Solver to use,The length of time to run the simulation(seconds),the time step(seconds)
%The minimum time step, the maximum time step
%Note: There are three solvers.
%      1. Fourth order variable time step Runge-Kutta method (number 0)
%      2. Fourth order fixed time step Runge-Kutta method (number 1)
%      3. Linear step Euler method (number 3)
time,0,10,0.001,1e-12,0.2

%The tolerances: prescribed accuracy,min element size,max element size
tol,,0.01,0.01,1

%Interface tension at an angle of zero degrees
g0,,100000

%Constant used to determine the interface tension
ki,,0

%Migration Mobility of grain boundary and difffusion mobility of pore
mob,,1, 0.0001, 1

%Node placements
%node,node id,x pos,y pos
%Node numbering must be 1, then 2, etc
%These MUST go in order clockwise
node,    1,-5,11
node,    2,-1,11
node,    3,1,11
node,    4,5,11
node,    5,1,10
node,    6,0,10
node,    7,-1,10
node,    8,0,11
node,    9,1,10.5
node,    10,-1,10.5



%Element placements
%elem,element id,node 1, node 2,Migration Mobility (0),Diffusion Mobility (1), fake element (2)
%Element numbering must be 1, then 2, etc. 
elem,    1,    1,   2,     1
elem,    2,    2,   8,     0
elem,    3,    3,    4,     1
elem,    4,    3,  9,     0
elem,    5,   5,  6,     0
elem,    6,   6,   7,     0
elem,    7,   7,   10,     0
elem,    8,   8,   3,     0
elem,    9,    9,  5,     0
elem,    10,    10,  2,     0
