%Solver to use,The length of time to run the simulation(seconds),the time step(seconds)
%The minimum time step, the maximum time step
%Note: There are three solvers.
%      1. Fourth order variable time step Runge-Kutta method (number 0)
%      2. Fourth order fixed time step Runge-Kutta method (number 1)
%      3. Linear step Euler method (number 3)
time,0,5,0.1,1e-12,0.2

%The tolerances: prescribed accuracy,min element size,max element size
tol,,0.01,0.01,1

%Interface tension at an angle of zero degrees
g0,,100000

%Constant used to determine the interface tension
ki,,0

%Migration Mobility of grain boundary and difffusion mobility of pore
mob,,1, 0.0001, 1

%Node placements
%node,node id,x pos,y pos
%Node numbering must be 1, then 2, etc
%These MUST go in order clockwise
node,	1	,	-1	,	0
node,	2	,	-1	,	-1.3
node,	3	,	0	,	-1.3
node,	4	,	1	,	-1.3
node,	5	,	1	,	0
node,	6	,	-5	,	0
node,	7	,	5	,	0
node,	8	,	-1	,	-0.433333
node,	9	,	-1	,	-0.866667
node,	10	,	-0.666667	,	-1.3
node,	11	,	-0.333333	,	-1.3
node,	12	,	0.333333	,	-1.3
node,	13	,	0.666667	,	-1.3
node,	14	,	1	,	-0.866667
node,	15	,	1	,	-0.433333
node,	16	,	-0.6	,	0
node,	17	,	-0.2	,	0
node,	18	,	0.2	,	0
node,	19	,	0.6	,	0
node,	20	,	-4.6	,	0
node,	21	,	-4.2	,	0
node,	22	,	-3.8	,	0
node,	23	,	-3.4	,	0
node,	24	,	-3	,	0
node,	25	,	-2.6	,	0
node,	26	,	-2.2	,	0
node,	27	,	-1.8	,	0
node,	28	,	-1.4	,	0
node,	29	,	1.4	,	0
node,	30	,	1.8	,	0
node,	31	,	2.2	,	0
node,	32	,	2.6	,	0
node,	33	,	3	,	0
node,	34	,	3.4	,	0
node,	35	,	3.8	,	0
node,	36	,	4.2	,	0
node, 	37	,	4.6	,	0




%Element placements
%elem,element id,node 1, node 2,Migration Mobility (0),Diffusion Mobility (1), fake element (2)
%Element numbering must be 1, then 2, etc. 
elem,    1,    1,    8,     1
elem,    2,    8,    9,     1
elem,    3,    9,    2,     1
elem,    4,    2,   10,     1
elem,    5,   10,   11,     1
elem,    6,   11,    3,     1
elem,    7,    3,   12,     1
elem,    8,   12,   13,     1
elem,    9,   13,    4,     1
elem,   10,    4,   14,     1
elem,   11,   14,   15,     1
elem,   12,   15,    5,     1
elem,   13,    1,   16,     1
elem,   14,   16,   17,     1
elem,   15,   17,   18,     1
elem,   16,   18,   19,     1
elem,   17,   19,    5,     1
elem,   18,    6,   20,     0
elem,   19,   20,   21,     0
elem,   20,   21,   22,     0
elem,   21,   22,   23,     0
elem,   22,   23,   24,     0
elem,   23,   24,   25,     0
elem,   24,   25,   26,     0
elem,   25,   26,   27,     0
elem,   26,   27,   28,     0
elem,   27,   28,    1,     0
elem,   28,    5,   29,     0
elem,   29,   29,   30,     0
elem,   30,   30,   31,     0
elem,   31,   31,   32,     0
elem,   32,   32,   33,     0
elem,   33,   33,   34,     0
elem,   34,   34,   35,     0
elem,   35,   35,   36,     0
elem,   36,   36,   37,     0
elem,   37,   37,    7,     0
